|  |
| --- |
| **Table 9.3.1.2 Criteria for assessable development** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Performance Outcomes** | **Examples that achieve aspects of the Performance Outcomes** | **E Compliance*** **Yes**
* **No See PO or**
* **NA**
 | **Justification for compliance** |
| **General criteria** |
| **Building height** |  |  |
| **PO1**Buildings have a height that:1. is consistent with the intended character of the streetscape, precinct and zone;
2. responds to the topographical features of the lot, including slope and orientation;
3. is not visually dominant or overbearing with respect to the streetscape.

|  |
| --- |
| Note - This is a qualitative statement that is an alternative provision to the QDC, part MP1.1, P4 and MP1.2, P4. |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | **E1**Building height does not exceed that mapped on Overlay map – Building heights.

|  |
| --- |
| Note - Minimum's mapped on Overlay map - Building heights, do not apply to Dwelling houses.Note - The above does not apply to domestic outbuildings. Refer to assessment criteria for Domestic outbuildings for requirements.Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A4 and part MP1.2, A4. Non-compliance with this provision for a Dwelling house requires a concurrence agency response from Council.  |

 |  |  |
| **PO2**Tall structures (e.g. antenna, aerial, chimney, flagpole, receiving dishes or the like) have a height and diameter that:1. is not visually dominant or overbearing with respect to the streetscape and the wider receiving environment;
2. does not adversely affect amenity of the area or of adjoining properties.
 | **E2**The height of tall structures (e.g. antenna, aerial, chimney, flagpole or the like) projects no more than 8.5m above the level of natural ground and transmission and receiving dishes are no larger than 1.2m diameter.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house requires a concurrence agency response from council.  |

 |  |  |
| **Setbacks** |  |  |
| **PO3**Dwelling houses([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) and structures are setback to: 1. be consistent with the intended character of the streetscape, precinct and zone;

|  |
| --- |
| Note - Refer to the overall outcomes for the relevant zone, precinct or sub-precinct to determine the relevant precinct character. |

1. ensure parked vehicles do not restrict pedestrian and traffic movement and safety;
2. provide adequate separation to particular infrastructure and waterbodies to minimise adverse impacts on people, property, water quality and infrastructure;
3. maintain the privacy of adjoining properties;
4. limit the length, height and openings of boundary walls to maximise privacy and amenity on adjoining properties;
5. ensure built to boundary walls do not create unusable or inaccessible spaces and do not negatively impact the streetscape character or the expected amenity of adjoining properties;
6. maintain private open space areas that are of a size and dimension to be useable and functional spaces.

|  |
| --- |
| Note - This is a qualitative statement that is an alternative provision to the QDC, part MP1.1, P1 and P2 and MP1.2, P1 and P2.  |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | **E3.1**Setbacks comply with:1. Emerging community zone:
	1. Transition precinct (developed lot) Morayfield South urban area identified in ‘Figure 9.3.1.1 Morayfield South - Urban area ’ - [Table 9.3.1.6 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.6)
	2. Transition precinct (developed lot) all other areas - [Table 9.3.1.5 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.5)
2. General residential zone:
	1. Coastal communities precinct - [Table 9.3.1.3 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.3)
	2. Suburban neighbourhood precinct - [Table 9.3.1.4 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.4)
	3. Next generation neighbourhood precinct - [Table 9.3.1.5 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.5)
	4. Urban neighbourhood precinct - [Table 9.3.1.6 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.6)
3. Caboolture West local plan:
	1. Urban living precinct - Next generation sub-precinct - [Table 9.3.1.5 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.5)
4. Redcliffe Kippa-Ring local plan:
	1. Interim residential precinct - [Table 9.3.1.3 ‘Setbacks’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.3)

|  |
| --- |
| Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A1 (a), (b) and (c), A2 (a), (b) and (d) and part MP1.2, A1 (a), (b) and (c), A2 (a), (b) and (d). Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) requires a concurrence agency response from Council.Note - Greater setbacks may be required if the lot adjoins an environmental corridor or area (Refer to values and constraints for details). Note - The above setbacks apply only to Class 1a and Class 10a buildings/structures. |

 |  |  |
| **E3.2**Built to boundary walls are:1. provided on lots with a frontage less than 18m, in accordance with aplan of development approved by council as part of a previous development approval applying to the land or as subsequently amended by council in writing;

OR1. for all other built to boundary walls refer to [Table 9.3.1.7 ‘Built to boundary walls’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.7) (mandatory/optional);
2. of a length and height in [Table 9.3.1.7 ‘Built to boundary walls’](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1360106863373#ID-327431-TABLE-9.3.1.7);
3. setback from the side boundary:
	1. not more than 20mm; or
	2. if a plan of development shows only one built to boundary wall on the boundary, not more than 200mm;
4. on the low side of a sloping lot.

|  |
| --- |
| Editor's note - Lots containing built to boundary walls should also include an appropriate easement to facilitate the maintenance of any wall within 600mm of a boundary.  For boundaries with built to boundary walls on adjacent lots a 'High Density Development Easement' is recommended; or for all other built to boundary walls a 'easement for maintenance purposes' is recommended.   |
|  Note - The above setbacks apply only to Class 1a and Class 10a buildings/structures.  |

|  |
| --- |
|  Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A1 (a), (b) and (c), A2 (a), (b) and (d) and part MP1.2, A1 (a), (b) and (c), A2 (a), (b) and (d). Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |
|  Editor's note - A wall is not to be built to the boundary if it has a window or if a wall of a building on an adjoining lot: 1. is within 900mm of that boundary;
2. is within 1.5m of that boundary and has an opening/window to a habitable room;
3. is not constructed from masonry or other material fire rated in accordance with the Building Code of Australia.
 |

 |  |  |
| **Site cover** |  |  |
| **PO4**Dwelling houses([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) and structures will ensure that site cover: 1. provides open areas around buildings for useable and functional private open space;
2. ensures that buildings and structures are consistent with the intended character of the area;
3. does not result in other elements of the site being compromised (e.g. setbacks, open space etc).

|  |
| --- |
| Note - This is a qualitative statement that is an alternative provision to the QDC, part MP1.1, P3 and MP1.2, P3. |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | **E4**Site cover (excluding eaves, sun shading devices, patios, balconies and other unenclosed structures) does not exceed:1. Emerging community zone:
	* Transition precinct (developed lot) - in accordance with the table below
2. General residential zone:
	* Coastal communities precinct – 50%
	* Suburban neighbourhood precinct – 50%
	* Next generation neighbourhood precinct – in accordance with the table below
	* Urban neighbourhood precinct – in accordance with the table below
3. Caboolture west local plan:
	* Urban living precinct - Next generation sub-precinct - in accordance with the table below
4. Redcliffe Kippa-Ring local plan:
	* Interim residential precinct - 50%

|  |  |
| --- | --- |
| **Building height** | **Lot Size** |
| **300m2 or less** | **301-400m2** | **401-500m2** | **501-1000m2** | **Greater than 1000m2** |
| 8.5m or less | 75% | 70% | 60% | 60% | 60% |
| >8.5m – 12.0m | 50% | 50% | 60% | 50% | 50% |
| >12.0m | N/A | N/A | N/A | 50% | 40% |
| Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A3 and part MP1.2, A3. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **Private open space** |  |  |
| **PO5**Dwellings are provided with private open space that is:1. of a size and dimension to be useable and functional;
2. directly accessible from the dwelling;
3. located so that residents and neighbouring properties experience a suitable level of residential amenity;
4. free of objects or structures that reduce or limit functionality.

|  |
| --- |
| Note - Dwelling houses([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) adjoining an arterial or sub-arterial road must not locate private open space areas adjoining or within the setback to that road. Refer to Overlay map - Road hierarchy for road classifications.  |
| Note - Utility areas (e.g. driveways, air-conditioning units, water tanks, clothes drying facility, storage structures, refuse storage areas and retaining structures) are to be shown on a site plan.  |

|  |
| --- |
| Note - Private open space areas may be included within an unenclosed living structure (e.g. patio). |
| Note - This is a qualitative standard that relates to the amenity and aesthetic impacts of the building or structure. |

 | No example provided. |  |  |
| **Car parking** |  |  |
| **PO6**Car parking is provided on-site that provides for the number and type of vehicles anticipated to access the lot and ensures a surplus of car parking is avoided.

|  |
| --- |
| Note - This is a qualitative statement that is an alternative provision to the QDC, part MP1.1, P8 and MP1.2, P8. |

 | **E6**Car parking spaces are provided in accordance with the table below.

|  |  |
| --- | --- |
| **Location** | **Minimum number of car spaces to be provided** |
| General residential zone:* Coastal communities precinct
* Suburban neighbourhood precinct

Redcliffe Kippa-Ring local plan:* Interim residential precinct
 | 3 per Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) |
| Emerging community zone:* Transition precinct (developed lot)

General residential zone:* Next generation neighbourhood precinct
* Urban neighbourhood precinct

Caboolture west local plan code:* Urban living precinct - Next generation sub-precinct
 | 1 per Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) |
|  Note - Does not include the parking of Heavy Vehicles or Heavy Machinery.  |

|  |
| --- |
|  Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A8 and par MP1.2, A8. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **PO7**Garages and carports facing a street are designed to:1. not dominate the street frontage;
2. maintain active frontages and opportunities for surveillance from within the dwelling;
3. contribute to the intended character of the streetscape;
4. be separated to facilitate on street parking.

|  |
| --- |
| Note - This is a qualitative standard that is an alternative provision to the QDC, part MP1.1, P1. |
| Note - This is a qualitative standard that relates to the amenity and aesthetic impacts of the building or structure. |

|  |
| --- |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | **E7**Garage and carport openings are in accordance with the table below:

|  |  |
| --- | --- |
| **Primary or Secondary frontage** | **Covered car space opening(s) per street frontage** |
| Greater than 18m | Not specified |
| Greater than 12.5m to 18m | 6m wide maximum |
| 12.5m\* or less | Single storey: 3.0m wide maximum;Two storey: 6.0m wide maximum and recessed 1.0m behind the front wall or balcony of upper level.

|  |
| --- |
| Editor's note - Front wall is to have a minimum length of 40% of the adjoining frontage. |

ORFor a laneway lot (Single or two storey): no maximum |
|  Note - \*For a laneway lot, vehicle access and parking must be provided via the laneway.  |

|  |
| --- |
|  Note - Refer to Planning scheme policy - Residential design for details and examples.  |
|  Note - For a Dwelling house on a lot under 450m2, this is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A1 (b). Non-compliance with this provision requires a concurrence agency response from Council.  |

|  |
| --- |
|  Note - For a Dwelling house on a lot of 450m2 or more, this is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision requires a concurrence agency response from Council.  |

 |  |  |
| **Access and driveways** |  |  |
| **PO8**Driveways, pedestrian entries and internal access ways are designed to: 1. provide lawful access;
2. not detract from the creation of active street frontages and positively contribute to the intended streetscape character;
3. provide a safe pedestrian environment;
4. not result in excessive crossovers and hardstand areas;
5. allows adequate space for on-street parking;
6. allows adequate space for street planting and street trees;
7. allow adequate space for garbage collection and the location of street infrastructure.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | **E8.1**Crossover widths are a maximum of 40% of the frontage access is being obtained from, or 4.8m whichever is the lesser, or for a laneway lot no maximum.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house requires a concurrence agency response from council.  |

 |  |  |
| **E8.2**Where there is a plan of development, driveway crossovers are located in accordance with a plan of development approved by Council as part of a development approval or as otherwise amended by Council in writing.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from council.  |

 |  |  |
| **E8.3**Driveways do not include a reversing bay, manoeuvring area or visitor parking spaces (other than tandem spaces) in the front setback.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **PO9**The driveway construction across the verge conforms to the relevant standard drawing for the classification of the road in accordance with Planning scheme policy - Integrated design.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | No example provided. |  |  |
| **PO10**Site access and driveways are designed and located in accordance with:1. where for a Council-controlled road, AS/NZS2890.1, section 3;
2. where for a State-controlled road, the Safe Intersection Sight Distance requirements in AustRoads and the appropriate IPWEAQ standard drawings, or a copy of a Transport Infrastructure Act, section 62 approval.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | No example provided. |  |  |
| **Screening – fences** |  |  |
| **PO11**Fencing and screening complements the streetscape character, contributes to privacy while maintaining surveillance between buildings and public spaces.

|  |
| --- |
| Note - The objective of providing surveillance of the street takes precedence over the provision of physical barriers for noise mitigation purposes. Where a barrier for noise is unavoidable it is to be aesthetically treated in accordance with an option detailed in Planning scheme policy - Residential design.  |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

|  |
| --- |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | No example provided. |  |  |
| **Casual surveillance** |  |  |
| **PO12**Buildings and structures are designed and oriented to have active frontages that provide visual interest, address road frontages and facilitate casual surveillance of all public spaces (streets, laneways, public open space areas, pedestrian paths and car parking areas) through: 1. incorporating habitable room windows and balconies that overlook public spaces including secondary frontages;
2. emphasising the pedestrian entry so that it is easily identifiable and safely accessible from the primary frontage.

|  |
| --- |
| Note - Dwelling houses([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) adjoining an arterial or sub-arterial road must address the arterial or sub-arterial road. Refer to Overlay map - Road hierarchy for road classifications.  |
| Note - Refer to State Government standards for CPTED. |

|  |
| --- |
| Note - Ground level dwellings at the front of the lot have individual access points to the street. |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | **E12.1**The Dwelling house (or the primary dwelling if including a secondary dwelling) must address primary frontages (excluding motorway and arterial roads) with a minimum of a front door, window(s) and pedestrian entrance.

|  |
| --- |
| Note - If an acoustic fence has been conditioned as part of a reconfiguring a lot approval this provision does not apply to that frontage.  |
|  Note - Refer to Overlay map - Road hierarchy for road classification.  |

|  |
| --- |
|  Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from council.  |

|  |
| --- |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 |  |  |
| **E12.2**A minimum of one habitable room window having an area of at least 1m2 on each level overlooks each adjoining public space (street, public open space or laneway).

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from council.  |

 |  |  |
| **Waste** |  |  |
| **PO13**Bins and bin storage areas are provided, designed and managed in accordance with Planning scheme policy – Waste.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | **E13**Each dwelling (primary and secondary) includes a bin storage area that:1. is not visible from public areas or screened from public areas;
2. is not located in the primary frontage setback, unless the dwelling is built to boundary on both sides of the lot with only one frontage;
3. is not located in an enclosed garage;
4. has a minimum area of 1m x 2m;
5. has access to the collection point without going through a dwelling (excluding a garage).

|  |
| --- |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |
|  Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from council.  |

 |  |  |
| **PO14**Waste storage areas are:1. not located in front of the main building line; or
2. are screened and aesthetically treated (e.g. with landscaping) to not dominate the streetscape.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |

 | No example provided. |  |  |

|  |  |  |
| --- | --- | --- |
| **Utilities** |  |  |
| **PO15**The dwelling is connected to:1. an existing reticulated electricity supply;
2. reticulated sewerage;
3. reticulated water;
4. dedicated and constructed road.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | **E15**The dwelling is connected to:1. an existing reticulated electricity supply;
2. reticulated sewerage where in a reticulated area;
3. reticulated water;
4. dedicated and constructed road.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from council.  |

 |  |  |
| **Sloping land** |  |  |
| **PO16**All earth retaining structures provide a positive interface with the streetscape and minimise impacts on the amenity of adjoining residents.

|  |
| --- |
| Note - This is a quantifiable standard that relates to the amenity and aesthetic impacts of the building or structure. |

 | **E16**Earth retaining structures:1. are not constructed of boulder rocks or timber;
2. where height is no greater than 900mm, are provided in accordance with Figure - Retaining on a boundary;

  **Figure - Retaining on boundary** Retaining on boundary1. where height is greater than 900mm but no greater than 1.5m, are to be setback at least the equivalent height of the retaining structure from any property boundary;
2. where height is greater than 1.5m, are to be setback and stepped 1.5m vertical: 1.5m horizontal, terraced, landscaped and drained as shown below.

**Figure - Cut** Cut**Figure - Fill** Fill

|  |
| --- |
| Note - This is a quantifiable standard that relates to the amenity and aesthetic impacts of the building or structure. |

 |  |  |
| **PO17**Development is designed to respond to sloping topography in the sitting, design and form of buildings and structures by:1. minimising overuse of cut and fill to create single flat pads and benching;
2. avoiding expanses of retaining walls, loss of trees and vegetation and interference with natural drainage systems;
3. minimising any impact on the landscape character of the zone;
4. protecting the amenity of adjoining properties.

|  |
| --- |
| Note - This is a quantifiable standard that relates to the amenity and aesthetic impacts of the building or structure. |

 | **E17.1**Building and lot design on slopes between 10% and 15% must: 1. avoid single-plane slabs and benching with the use of split-level, multiple-slab, pier or pole construction;
2. have built to boundary walls on the low side of the lot to avoid drainage issues.

|  |
| --- |
| Note - This is a quantifiable standard that relates to the amenity and aesthetic impacts of the building or structure. |

 |  |  |
| **E17.2**New buildings on land with a slope greater than 15% do not have slab on ground construction.

|  |
| --- |
| Note - This is a quantifiable standard that relates to the amenity and aesthetic impacts of the building or structure. |

 |  |  |
| **Development on a laneway** |  |  |
| **PO18**Where a lot has a non-laneway frontage, the dwelling is designed and orientated towards the non-laneway frontage e.g. Street or park) and incorporates design elements to address and activate the non-laneway frontage (e.g. front door, windows, low front fencing (if any) with a gate etc).

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | **E18**The Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) (or the primary dwelling where including a secondary dwelling) 1. faces the non-laneway frontage;
2. has its main pedestrian entrance (front door) from the non-laneway frontage.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **PO19**All vehicle access must be via the laneway.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | No example provided. |  |  |
| **PO20**Dwelling houses([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) on laneways contribute to the streetscape by: 1. providing concealed garbage bin storage areas to reduce the dominance of bins on the lane;
2. maximising security and amenity;
3. including landscaping that:
	1. does not provide areas of concealment;
	2. breaks up the dominance of garages and vehicle parking;
	3. delineates the boundaries between lots.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | No example provided. |  |  |
| **Secondary dwelling** |  |  |
| **PO21**Secondary dwellings:1. are subordinate and ancillary to the primary dwelling in size and function;
2. have a GFA that does not exceed:
	1. 45m2 for a lot with a primary frontage less than 15m; or
	2. 55m2 for a lot with a primary frontage of 15m or more.
3. have the appearance, bulk and scale of a single dwelling from the street;
4. maintain sufficient area for the siting of all buildings, structures, landscaping and car parking spaces for the Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512)) on the lot.

|  |
| --- |
| Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | **E21.1**The siting and design of dwellings ensures that the secondary dwelling is:1. not located in front of the primary dwelling;
2. annexed to (adjoining, below or above) or located within 10.0m of the primary dwelling (excluding domestic outbuildings).

|  |
| --- |
| Note - Refer to Planning scheme policy - Residential design for details and examples. |
|  Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from council.  |

 |  |  |
| **E21.2**No more than 1 secondary dwelling is located on an allotment.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **E21.3**The GFA of the secondary dwelling does not exceed:1. 45m2 GFA for a lot with a primary frontage less than 15m; or
2. 55m2 GFA for a lot with a primary frontage of 15m or more.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **E21.4**Where additional car parking spaces are provided, car parking spaces are co-located with the parking spaces for the primary dwelling to appear as a single dwelling from the street.

|  |
| --- |
| Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.  |

 |  |  |
| **Domestic outbuildings** |  |  |
| **PO22**Domestic outbuildings and car ports are:1. of a height that does not negatively impact the visual amenity of adjoining properties;
2. located on-site to not dominate the streetscape.

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian.Note - This is a qualitative standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. |

 | **E22**Domestic outbuildings:1. have a total combined maximum roofed area as outlined in the table below:

|  |  |
| --- | --- |
| **Size of lot** | **Maximum roofed area** |
| Less than 600m2 | 50m2 |
| 600m2 - 1000m2 | 70m2 |
| >1000m2 – 2000m2 | 80m2 |
| Greater than 2000m2 | 150m2 |

1. have a maximum building height of 4m and a mean height not exceeding 3.5m;
2. are located behind the main building line and not within primary or secondary frontage setbacks.

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian.Note - This is a quantifiable standard that relates to matters identified in Schedule 9, Part 3, Division 2, Table of Regulation. Non-compliance with this provision for a Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) requires a concurrence agency response from Council.Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A4 and part MP1.2, A4. Non-compliance with this provision for a Dwelling house requires a concurrence agency response from Council. Note - This is a quantifiable standard that is an alternative provision to the QDC, part MP1.1, A1 (a), (b) and (c), A2 (a), (b) and (d) and part MP1.2, A1 (a), (b) and (c), A2 (a), (b) and (d). Non-compliance with this provision for a Dwelling houserequires a concurrence agency response from Council. Note - Greater setbacks may be required if the lot adjoins an environmental corridor or area (Refer to values and constraints for details).  |

 |  |  |

|  |  |
| --- | --- |
| **Values and constraints criteria**

|  |
| --- |
| Note - The relevant values and constraints criteria do not apply where the development is consistent with a current Development permit for Reconfiguring a lot or Material change of use or Operational work, where that approval has considered and addressed (e.g. through a development footprint plan (or similar in the case of Landslide hazard) or conditions of approval) the identified value or constraint under this planning scheme.  |

 |
| **Acid sulfate soils - (refer Overlay map - Acid sulfate soils to determine if the following assessment criteria apply)**

|  |
| --- |
| Note - To demonstrate achievement of the performance outcome, an Acid sulfate soils (ASS) investigation report and soil management plan is prepared by a qualified engineer.  Guidance for the preparation an ASS investigation report and soil management plan is provided in Planning scheme policy - Acid sulfate soils.  |

 |
| **PO23**Development avoids disturbing acid sulfate soils. Where development disturbs acid sulfate soils, development:1. is managed to avoid or minimise the release of surface or groundwater flows containing acid and metal contaminants into the environment;
2. protects the environmental and ecological values and health of receiving waters;
3. protects buildings and infrastructure from the effects of acid sulfate soils.
 | **E23**Development does not involve:1. excavation or otherwise removing of more than 100m3 of soil or sediment where below than 5m Australian Height datum AHD; or
2. filling of land of more than 500m3 of material with an average depth of 0.5m or greater where below the 5m Australian Height datum AHD.
 |  |  |
| **Environmental areas (refer Overlay map - Environmental areas to determine if the following assessment criteria apply)**

|  |
| --- |
| Note – The following are excluded from the native vegetation clearing provisions of this planning scheme:1. Clearing of native vegetation located within an approved development footprint;
2. Clearing of native vegetation within 10m from a lawfully established building reasonably necessary for emergency access or immediately required in response to an accident or emergency;
3. Clearing of native vegetation reasonably necessary to remove or reduce the risk vegetation poses to serious personal injury or damage to infrastructure;
4. Clearing of native vegetation reasonably necessary to construct and maintain a property boundary fence and not exceed 4m in width either side of the fence where in the Rural, Rural residential and Environmental Management and Conservation zones.  In any other zone, clearing is not to exceed 2m in width either side of the fence;
5. Clearing of native vegetation reasonably necessary for the purpose of maintenance or works within a registered easement for public infrastructure or drainage purposes;
6. Clearing of native vegetation in accordance with a bushfire management plan prepared by a suitably qualified person, submitted to and accepted by Council;
7. Clearing of native vegetation associated with removal of recognised weed species, maintaining existing open pastures and cropping land, windbreaks, lawns or created gardens;
8. Grazing of native pasture by stock;
9. Native forest practice where accepted development under Part 1, 1.7.7 Accepted development
 |
| Note - Definition for native vegetation is located in Schedule 1 Definitions.Note - Native vegetation subject to this criteria primarily comprises of matters of national environmental significance (MNES), matters of state environmental significance (MSES).  They also comprise some matters of local environmental significance (MLES). A MLES is defined in Schedule 1.2, Administrative definitions. A list of the elements that apply to the mapped MSES and MLES is provided in Appendix 1 of the Planning scheme policy - Environmental areas. Editors' Note - The accuracy of overlay mapping can be challenged through the development application process (code assessable development) or by way of a planning scheme amendment. See Council's website for details.  |

|  |
| --- |
| Note - To demonstrate achievement of the performance outcome, an ecological assessment, vegetation management plan and fauna management plan, as required, are prepared by a suitably qualified person.  Guidance for the preparation of above mentioned reports is provided in Planning scheme policy - Environmental areas.  |

 |
| **Vegetation clearing, ecological value and connectivity** |  |  |
| **PO24**Development avoids locating in a High Value Area or a Value Offset Area.  Where it is not practicable or reasonable for development to avoid establishing in these areas, development must ensure that: 1. the quality and integrity of the biodiversity and ecological values inherent to a High Value Area and a Value Offset Area is maintained and not lost or degraded;
2. on-site mitigation measures, mechanisms or processes are in place demonstrating the quality and integrity of the biodiversity and ecological values inherent to a High Value Area and a Value Offset Area are maintained.  For example, this can be achieved through replacement, restoration or rehabilitation planting as part of any proposed covenant,  the development of a Vegetation Management Plan,  a Fauna Management Plan, and any other on-site mitigation options identified in the Planning scheme policy - Environmental areas\*.

|  |
| --- |
| \* Editor's note - This is not a requirement for an environmental offset under the Environmental Offsets Act 2014. |

 | No example provided. |  |  |
| **PO25**Development provides for safe, unimpeded, convenient and ongoing wildlife movement and establishes and maintains habitat connectivity by: 1. retaining habitat trees;
2. providing contiguous patches of habitat;
3. provide replacement and rehabilitation planting to improve connectivity;
4. avoiding the creation of fragmented and isolated patches of habitat;
5. providing wildlife movement infrastructure.

|  |
| --- |
| Editor's note - Wildlife movement infrastructure may include refuge poles, tree boulevarding, ‘stepping stone’ vegetation plantings, tunnels, appropriate wildlife fencing; culverts with ledges, underpasses, overpasses, land bridges and rope bridges. Further information is provided in Planning scheme policy – Environmental areas.  |

 | No example provided. |  |  |
| **Vegetation clearing and habitat protection** |  |  |
| **PO26**Development ensures that the biodiversity quality and integrity of habitats is not adversely impacted upon but maintained and protected.  | No example provided. |  |  |
| **PO27**Development does not result in the net loss or degradation of habitat value in a High Value Area or a Value Offset Area.  Where development does result in the loss or degradation of habitat value, development will: 1. rehabilitate, revegetate, restore and enhance an area to ensure it continues to function as a viable and healthy habitat area;
2. provide replacement fauna nesting boxes in the event of habitat tree loss in accordance with Planning scheme policy - Environmental areas;
3. undertake rehabilitation, revegetation and restoration in accordance with the South East Queensland Ecological Restoration Framework.
 | No example provided. |  |  |
| **PO28**Development ensures safe, unimpeded, convenient and ongoing wildlife movement and habitat connectivity by:1. providing contiguous patches of habitat;
2. avoiding the creation of fragmented and isolated patches of habitat;
3. providing wildlife movement infrastructure;
4. providing replacement and rehabilitation planting to improve connectivity.
 | No example provided. |  |  |
| **Vegetation clearing and soil resource stability** |  |  |
| **PO29**Development does not:1. result in soil erosion or land degradation;
2. leave cleared land exposed for an unreasonable period of time but is rehabilitated in a timely manner.
 | No example provided. |  |  |
| **Vegetation clearing and water quality** |  |  |
| **PO30**Development maintains or improves the quality of groundwater and surface water within, and downstream, of a site by:1. ensuring an effective vegetated buffers and setbacks from waterbodies is retained to achieve natural filtration and reduce sediment loads;
2. avoiding or minimising changes to landforms to maintain hydrological water flows;
3. adopting suitable measures to exclude livestock from entering a waterbody where a site is being used for animal husbandry([4](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447116)) and animal keeping([5](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447140)) activities.
 | No example provided. |  |  |
| **PO31**Development minimises adverse impacts of stormwater run-off on water quality by:1. minimising flow velocity to reduce erosion;
2. minimising hard surface areas;
3. maximising the use of permeable surfaces;
4. incorporating sediment retention devices;
5. minimising channelled flow.
 | No example provided. |  |  |
| **Vegetation clearing and access, edge effects and urban heat island effects** |  |  |
| **PO32**Development retains safe and convenient public access in a manner that does not result in the adverse edge effects or the loss or degradation of biodiversity values within the environment.  | No example provided. |  |  |
| **PO33**Development minimises potential adverse ‘edge effects’ on ecological values by:1. providing dense planting buffers of native vegetation between a development and environmental areas;
2. retaining patches of native vegetation of greatest possible size where located between a development and environmental areas ;
3. restoring, rehabilitating and increasing the size of existing patches of native vegetation;
4. ensuring that buildings and access (public and vehicle) are setback as far as possible from environmental areas and corridors;
5. landscaping with native plants of local origin.

|  |
| --- |
| Editor's note - Edge effects are factors of development that go to detrimentally affecting the composition and density of natural populations at the fringe of natural areas. Factors include weed invasion, pets, public and vehicle access, nutrient loads, noise and light pollution, increased fire frequency and changes in the groundwater and surface water flow.  |

 | No example provided. |  |  |
| **PO34**Development avoids adverse microclimate change and does not result in increased urban heat island effects.  Adverse urban heat island effects are minimised by: 1. pervious surfaces;
2. providing deeply planted vegetation buffers and green linkage opportunities;
3. landscaping with local native plant species to achieve well-shaded urban places;
4. increasing the service extent of the urban forest canopy.
 | No example provided. |  |  |
| **Vegetation clearing and Matters of Local Environmental Significance (MLES) environmental offsets** |  |  |
| **PO35**Where development results in the unavoidable loss of native vegetation within a Value Offset Area MLES waterway buffer or a Value Offset Area MLES wetland buffer, an environmental offset is required in accordance with the environmental offset requirements identified in Planning scheme policy - Environmental areas.

|  |
| --- |
| Editor's note - For MSES Koala Offsets, the environmental offset provisions in Schedule 11 of the Regulation, in combination with the requirements of the Environmental Offsets Act 2014, apply.  |

 | No example provided. |  |  |
| **Extractive resources separation area (refer Overlay map - Extractive resources (separation area) to determine if the following assessment criteria apply)**

|  |
| --- |
| Note - To demonstrate achievement of the performance outcomes, a noise impact assessment report is prepared by a suitably qualified person. Guidance to preparing noise impact assessment report is provided in Planning scheme policy – Noise.  |

 |
| **PO36**Development does not increase the number of people living in the Extractive Resources separation area. | **E36**One dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181" \l "target-d60297e447512" \o "Dwelling house - A residential use of premises for one household that contains a single dwelling.  The use includes residential outbuildings and works normally associated with a dwelling and may include a secondary dwelling.)) permitted per lot within separation area.  |  |  |
| **PO37**Development:1. does not introduce or increase uses that are sensitive to the impacts of an Extractive industry([27](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447616));
2. is compatible with the operation of an Extractive industry([27](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447616));
3. does not comprise or undermine the function and integrity of the separation area in providing a buffer between key extractive and processing activities and sensitive, incompatible uses outside the separation area.
 | **E37**Development within the separation area does not include the following activities:1. Caretaker's accommodation([10](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447244));
2. Community residence([16](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447372));
3. Dual occupancy([21](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447482));
4. Dwelling unit([23](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447532));
5. Hospital([36](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447830));
6. Rooming accommodation([69](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448729));
7. Multiple dwelling([49](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448163));
8. Non-resident workforce accommodation([52](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448245));
9. Relocatable home park([62](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448511));
10. Residential care facility([65](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448576));
11. Resort complex([66](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448613));
12. Retirement facility([67](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448657));
13. Rural workers’ accommodation([71](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448803));
14. Short-term accommodation([77](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448936));
15. Tourist park([84](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449196)).
 |  |  |
| **PO38**Habitable rooms achieve the noise levels listed in Schedule 1 Acoustic Quality Objectives, Environmental Protection (Noise) Policy 2008 and provides a safe, healthy and disturbance free living environment.  | **E38**All habitable rooms within the separation area are:1. acoustically insulated to achieve the noise levels listed in Schedule 1 Acoustic Quality Objectives, Environmental Protection (Noise) Policy 2008;
2. provided with mechanical ventilation.
 |  |  |
| **PO39**Development provides open space areas for passive recreation in a manner where impacts from key extractive/processing activities, particularly noise, is minimised.  | **E39**Private open space areas are separated from the resource processing area by buildings or a 1.8m high solid structure. |  |  |
| **Extractive resources transport route (refer Overlay map - Extractive resources (transport route and buffer) to determine if the following assessment criteria apply)** |
| **PO40**Development:1. does not increase in the number of people living in close proximity to a transport route and being subject to the adverse effects from the transportation route;
2. does not result in the establishment of uses that are incompatible with the operation of Extractive resources transport routes;
3. adopts design and location measures to satisfactorily mitigate the potential adverse impacts associated with transportation routes on sensitive land uses.  Such measures include, but are not limited to:
	1. locating the furthest distance possible from the transportation route;
	2. habitable rooms being located the furthest from the transportation route;
	3. shielding and screening private outdoor recreation space from the transportation routes.
 | **E40**The following uses are not located within the 100m wide transport route buffer:1. Caretaker’s accommodation([10](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447244)), except where located in the Extractive industry zone;
2. Community residence([16](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447372));
3. Dual occupancy([21](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447482));
4. Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512));
5. Dwelling unit([23](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447532));
6. Hospital([36](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447830));
7. Rooming accommodation([69](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448729));
8. Multiple dwelling([49](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448163));
9. Non-resident workforce accommodation([52](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448245));
10. Relocatable home park([62](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448511));
11. Residential care facility([65](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448576));
12. Resort complex([66](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448613));
13. Retirement facility([67](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448657));
14. Rural workers’ accommodation([71](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448803));
15. Short-term accommodation([77](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448936));
16. Tourist park([84](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449196)).
 |  |  |
| **PO41**Development:1. does not adversely impact upon the efficient and effective transportation of extractive material along a transportation route;
2. ensures vehicle access and egress along transportation routes are designed and located to achieve a high degree of safety, having good visibility;
3. utilises existing vehicle access points and where existing vehicle access points are sub-standard or poorly formed, they are upgraded to an appropriate standard.
 | **E41.1**Development does not create a new vehicle access point onto an Extractive resources transport route. |  |  |
| **E41.2**A vehicle access point is located, designed and constructed in accordance with Planning scheme policy - Integrated design. |  |  |
| **Heritage and landscape character (refer Overlay map - Heritage and landscape character to determine if the following assessment criteria apply)**

|  |
| --- |
| Note - To assist in demonstrating achievement of heritage performance outcomes, a Cultural heritage impact assessment report is prepared by a suitably qualified person verifying the proposed development is in accordance with The Australia ICOMOS Burra Charter. Note - To assist in demonstrating achievement of this performance outcome, a Tree assessment report is prepared by a qualified arborist in accordance with Planning scheme policy – Heritage and landscape character.  The Tree assessment report will also detail the measures adopted in accordance with AS 4970-2009 Protection of trees on development sites. Note - Places, including sites, objects and buildings having local cultural heritage significance, are identified on Overlay map - Heritage and landscape character and listed in Schedule 1 of Planning scheme policy - Heritage and landscape character.  Places also having cultural heritage significance at a State level and being entered in the Queensland Heritage Register, are also identified in Schedule 1 of Planning scheme policy - Heritage and landscape character.  |

 |
| **PO42**Development will:1. not diminish or cause irreversible damage to the cultural heritage values present on the site, and associated with a heritage site, object or building;
2. protect the fabric and setting of the heritage site, object or building;
3. be consistent with the form, scale and style of the heritage site, object or building;
4. utilise similar materials to those existing, or where this is not reasonable or practicable, neutral materials and finishes;
5. incorporate complementary elements, detailing and ornamentation to those present on the heritage site, object or building;
6. retain public access where this is currently provided.
 | **E42**Development is for the preservation, maintenance, repair and restoration of a site, object or building of cultural heritage value.

|  |
| --- |
| Note - A cultural heritage conservation management plan for the preservation, maintenance, repair and restoration of a site, object or building of cultural heritage value is prepared in accordance with Planning scheme policy - Heritage and landscape character. The plan is sent to, and approved by Council prior to the commencement of any preservation, maintenance, repair and restoration works.  |

 |  |  |
| **PO43**Demolition and removal is only considered where:1. a report prepared by a suitably qualified conservation architect or conservation engineer demonstrates that the building is structurally unsound and is not reasonably capable of economic repair; or
2. demolition is confined to the removal of outbuildings, extensions and alterations that are not part of the original structure; or
3. limited demolition is performed in the course of repairs, maintenance or restoration; or
4. demolition is performed following a catastrophic event which substantially destroys the building or object.
 | No example provided. |  |  |
| **PO44**Where development is occurring on land adjoining a site of cultural heritage value, the development is to be sympathetic to and consistent with the cultural heritage values present on the site and not result in their values being eroded, degraded or unreasonably obscured from public view.  | No example provided. |  |  |
| **PO45**Development does not adversely impact upon the health and vitality of significant trees. Where development occurs in proximity to a significant tree, construction measures and techniques as detailed in AS 4970-2009 Protection of trees on development sites are adopted to ensure a significant tree's health, wellbeing and vitality. Significant trees are only removed where they are in a poor state of health or where they pose a health and safety risk to persons or property. A Tree Assessment report prepared by a suitably qualified arborist confirming a tree's state of health is required to demonstrate achievement of this performance outcome.  | **E45**Development does:1. not result in the removal of a significant tree;
2. not occur within 20m of a protected tree;
3. involve pruning of a tree in accordance with Australian Standard AS 4373-2007 – Pruning of Amenity Trees.
 |  |  |
| **Infrastructure buffers (refer Overlay map - Infrastructure buffers to determine if the following assessment criteria apply)** |
| **PO46**Odour sensitive development is separated from Wastewater treatment plants so they are not adversely affected by odour emission or other air pollutant impacts.  | **E46**The following uses are not located within a wastewater treatment site buffer:1. Caretaker’s accommodation([10](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447244));
2. Community residence([16](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447372));
3. Dual occupancy([21](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447482));
4. Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512))
5. Dwelling unit([23](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447532));
6. Hospital([36](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447830));
7. Rooming accommodation([69](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448729));
8. Multiple dwelling([49](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448163));
9. Non-resident workforce accommodation([52](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448245));
10. Relocatable home park([62](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448511));
11. Residential care facility([65](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448576));
12. Resort complex([66](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448613));
13. Retirement facility([67](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448657));
14. Rural workers’ accommodation([71](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448803));
15. Short-term accommodation([77](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448936));
16. Tourist park([84](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449196)).
 |  |  |
| **PO47**Development within a Bulk water supply infrastructure buffer is located, designed and constructed to:1. protect the integrity of the water supply pipeline;
2. maintain adequate access for any required maintenance or upgrading work to the water supply pipeline;
 | **E47**Development:1. does not involve the construction of any buildings or structures within a Bulk water supply infrastructure buffer;
2. involving a major hazard facility or environmentally relevant activity (ERA) is setback 30m from a Bulk water supply infrastructure buffer.
 |  |  |
| **PO48**Development is located and designed to maintain required access to Bulk water supply infrastructure. | **E48**Development does not restrict access to Bulk water supply infrastructure of any type or size, having regard to (among other things): 1. buildings or structures;
2. gates and fences;
3. storage of equipment or materials;
4. landscaping or earthworks or stormwater or other infrastructure.
 |  |  |
| **PO49**Development within the Gas pipeline buffer:1. avoids attracting people in large numbers to live, work or congregate;
2. avoids the storage of hazardous chemicals;
3. maintains adequate access for any required maintenance or upgrading work;
4. minimises risk of harm to people and property.

|  |
| --- |
| Editor's note - The *Petroleum and Gas (Production and Safety) Act 2004* (sections 807 and 808) requires that building or changes in surface level on pipeline land must not occur unless all the pipeline licence holders consent.  |

 | **E49**Development does not involve the construction of any buildings or structures within the Gas pipeline buffer.

|  |
| --- |
| Editor's note - The *Petroleum and Gas (Production and Safety) Act 2004* (sections 807 and 808) requires that building or changes in surface level on pipeline land must not occur unless all the pipeline licence holders consent.  |

 |  |  |
| **PO50**Odour sensitive development is separated from landfill sites so they are not adversely affected by odour emission or other air pollutant impacts.  | **E50**The following uses are not located within a Landfill buffer:1. Caretaker’s accommodation([10](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447244));
2. Community residence([16](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447372));
3. Dual occupancy([21](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447482));
4. Dwelling house([22](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447512));
5. Dwelling unit([23](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447532));
6. Hospital([36](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e447830));
7. Rooming accommodation([69](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448729));
8. Multiple dwelling([49](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448163));
9. Non-resident workforce accommodation([52](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448245));
10. Relocatable home park([62](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448511));
11. Residential care facility([65](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448576));
12. Resort complex([66](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448613));
13. Retirement facility([67](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448657));
14. Rural workers’ accommodation([71](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448803));
15. Short-term accommodation([77](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448936));
16. Tourist park([84](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449196)).
 |  |  |
| **PO51**Habitable rooms within an Electricity supply substation buffer are located a sufficient distance from substations([80](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449077)) to avoid any potential adverse impacts on personal health and wellbeing from electromagnetic fields.

|  |
| --- |
| Note - Habitable room is defined in the Building Code of Australia (Volume 1) |

 | **E51**Habitable rooms:1. are not located within an Electricity supply substation buffer; and
2. proposed on a site subject to an Electricity supply supply substation([80](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449077))are acoustically insulted to achieve the noise levels listed in Schedule 1, Acoustic Quality Objectives, Environmental Protection (Noise) Policy 2008.

|  |
| --- |
| Note - Habitable room is defined in the Building Code of Australia (Volume 1) |

 |  |  |
| **PO52**Habitable rooms within an Electricity supply substation buffer are acoustically insulated from the noise of a substation([80](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e449077)) to achieve the noise levels listed in Schedule 1 Acoustic Quality Objectives, Environmental Protection (Noise) Policy 2008 and provides a safe, healthy and disturbance free living environment.

|  |
| --- |
| Note - To demonstrate achievement of the performance outcome, a noise impact assessment report is prepared by a suitably qualified person. Guidance to preparing an noise impact assessment report is provided in Planning scheme policy – Noise.  |
| Note - Habitable room is defined in the Building Code of Australia (Volume 1) |

 | No example provided. |  |  |
| **PO53**Development within a High voltage electricity line buffer provides adequate buffers to high voltage electricity lines to protect amenity and health by ensuring development: 1. is located and designed to avoid any potential adverse impacts on personal health and wellbeing from electromagnetic fields in accordance with the principle of prudent avoidance;
2. is located and designed in a manner that maintains a high level of  security of supply;
3. is located and design so not to impede upon the functioning and maintenance of high voltage electrical infrastructure.
 | **E53**Development does not involve the construction of any buildings or structures within a High voltage electricity line buffer. |  |  |
| **Overland flow path (refer Overlay map - Overland flow path to determine if the following assessment criteria apply)**

|  |
| --- |
| Note - The applicable river and creek flood planning levels associated with defined flood event (DFE) within the inundation area can be obtained by requesting a flood check property report from Council.  |

 |
| **PO54**Development:1. minimises the risk to persons from overland flow;
2. does not increase the potential for damage from overland flow either on the premises or other premises, public land, watercourses, roads or infrastructure.
 | No example provided. |  |  |
| **PO55**Development:1. maintains the conveyance of overland flow predominantly unimpeded through the premises for any event up to and including the 1% AEP for the fully developed upstream catchment;
2. does not concentrate, intensify or divert overland flow onto an upstream, downstream or surrounding property.

|  |
| --- |
| Note - A report from a suitably qualified Registered Professional Engineer Queensland is required certifying that the development does not increase the potential for significant adverse impacts on an upstream, downstream or surrounding premises.  |
| Note - Reporting to be prepared in accordance with Planning scheme policy – Flood hazard, Coastal hazard and Overland flow. |

 | **E55**No example provided. |  |  |
| **PO56**Development does not:1. directly, indirectly or cumulatively cause any increase in overland flow velocity or level;
2. increase the potential for flood damage from overland flow either on the premises or other premises, public lands, watercourses, roads or infrastructure.

|  |
| --- |
| Note - Open concrete drains greater than 1m in width are not an acceptable outcome, nor are any other design options that may increase scouring.  |

 | No example provided. |  |  |
| **PO57**Development ensures that public safety and the risk to the environment are not adversely affected by a detrimental impact of overland flow on a hazardous chemical located or stored on the premises.  | **E57**Development ensures that a hazardous chemical is not located or stored in an Overland flow path area.

|  |
| --- |
| Note - Refer to the Work Health and Safety Act 2011 and associated Regulation and Guidelines, the Environmental Protection Act 1994 and the relevant building assessment provisions under the Building Act 1975 for requirements related to the manufacture and storage of hazardous substances.  |

 |  |  |
| **PO58**Development which is not in a Rural zone ensures that overland flow is not conveyed from a road or public open space onto a private lot.  | **E58**Development which is not in a Rural zone that an overland flow paths and drainage infrastructure is provided to convey overland flow from a road or public open space area away from a private lot.  |  |  |
| **PO59**Development ensures that inter-allotment drainage infrastructure, overland flow paths and open drains through private property cater for overland flows for a fully developed upstream catchment and are able to be easily maintained.

|  |
| --- |
| Note - A report from a suitably qualified Registered Professional Engineer Queensland is required certifying that the development does not increase the potential for significant adverse impacts on an upstream, downstream or surrounding premises.  |
| Note - Reporting to be prepared in accordance with Planning scheme policy – Flood hazard, Coastal hazard and Overland flow |

 | **E59.1**Development ensures that roof and allotment drainage infrastructure is provided in accordance with the following relevant level as identified in QUDM: 1. Urban area – Level III;
2. Rural area – N/A;
3. Industrial area – Level V;
4. Commercial area – Level V.
 |  |  |
| **E59.2**Development ensures that inter-allotment drainage infrastructure is designed to accommodate any event up to and including the 1% AEP for the fully developed upstream catchment.  |  |  |
| **PO60**Development protects the conveyance of overland flow such that an easement for drainage purposes is provided over:1. a stormwater pipe if the nominal pipe diameter exceeds 300mm;
2. an overland flow path where it crosses more than one premises;
3. inter-allotment drainage infrastructure.

|  |
| --- |
| Note - Refer to Planning scheme policy - Integrated design for details and examples. |
| Note - Stormwater Drainage easement dimensions are provided in accordance with Section 3.8.5 of QUDM. |

 | No example provided. |  |  |
| **Additional criteria for development for a Park(**[57](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448382)**)** |  |  |
| **PO61**Development for a Park([57](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448382)) ensures that the design and layout responds to the nature of the overland flow affecting the premises such that: 1. public benefit and enjoyment is maximised;
2. impacts on the asset life and integrity of park structures is minimised;
3. maintenance and replacement costs are minimised.
 | **E61**Development for a Park([57](http://consult.moretonbay.qld.gov.au/portal/mbrcpsv3?pointId=s1332743658181#target-d60297e448382)) ensures works are provided in accordance with the requirements set out in Appendix B of the Planning scheme policy - Integrated design.  |  |  |
| **Riparian and wetland setbacks** |  |  |
| **PO62**Development provides and maintains a suitable setback from waterways and wetlands that protects natural and environmental values.  This is achieved by recognising and responding to the following matters: 1. impact on fauna habitats;
2. impact on wildlife corridors and connectivity;
3. impact on stream integrity;
4. impact of opportunities for revegetation and rehabilitation planting;
5. edge effects.
 | **E62**Development does not occur within:1. 50m from top of bank for W1 waterway and drainage line
2. 30m from top of bank for W2 waterway and drainage line
3. 20m from top of bank for W3 waterway and drainage line
4. 100m from the edge of a Ramsar wetland, 50m from all other wetlands.

|  |
| --- |
| Note - W1, W2 and W3 waterway and drainage lines, and wetlands are mapped on Schedule 2, Section 2.5 Overlay Maps – Riparian and wetland setbacks.  |

 |  |  |
| **Scenic amenity - Regionally significant (Hills) and Locally important (Coast) (refer Overlay map - Scenic amenity to determine if the following assessment criteria apply)** |
| **PO63**Development:1. avoids being viewed as a visually conspicuous built form on a hill top or ridgeline;
2. retain the natural character or bushland settings as the dominant landscape characteristic;
3. is viewed as being visually consistent with the natural landscape setting and does not diminish the scenic and visual qualities present in the environment.
 | **E63**Where located in the Regionally significant (Hills) scenic amenity overlay, buildings and structures are not:1. located on a hill top or ridge line;
2. all parts of the building and structure are located below the hill top or ridge line.
 |  |  |
| **PO64**Development:1. does not adversely detract or degrade the quality of views, vista or key landmarks;
2. retains the natural character or bushland settings as the dominant landscape characteristic.
 | **E64**Where located in the Regionally significant (Hills) scenic amenity overlay, driveways and accessways:1. go across land contours, and do not cut straight up slopes;
2. follow natural contours, not resulting in batters or retaining walls being greater than 900mm in height.
 |  |  |
| **PO65**Buildings and structures incorporate colours and finishes that:1. are consistent with a natural, open space character and bushland environment;
2. do not produce glare or appear visual incompatible with the surrounding natural character and bushland environment;
3. are not visually dominant or detract from the natural qualities of the landscape.
 | **E65.1**Where located in the Regionally significant (hills) scenic amenity overlay, roofs and wall surfaces of buildings and structures adopt the following colours:

|  |
| --- |
| **Colours from Australian Standard AS2700s – 1996** |
| G12 – Holly | G54 – Mist Green | N 44 – Bridge Grey |
| G13 – Emerald | G55 – Lichen | N45 – Koala Grey |
| G14 – Moss Green | G56 – Sage Green | N52 – Mid Grey |
| G15 – Rainforest Green | G62 – Rivergum | N54 – Basalt |
| G16 – Traffic Green | G64 – Slate | N55 – Lead Grey |
| G17 – Mint Green | G65 – Ti Tree | X54 – Brown |
| G21 – Jade | N25 – Birch Grey | X61 – Wombat |
| G22 – Serpentine | N32 – Green Grey | X62 – Dark Earth |
| G23 – Shamrock | N33 – Lightbox Grey | X63 – Iron Bark |
| G24 – Fern Green | N35 – Light Grey | Y51 – Bronze Olive |
| G25 – Olive | N41 – Oyster | Y61 – Black Olive |
| G34 – Avocado | N42 – Storm Grey | Y63 – Khaki |
| G52 – Eucalyptus | N43 – Pipeline Grey | Y66 – Mudstone |
| G53 – Banksia |   |   |

 |  |  |
| **E65.2**Where located in the Regionally significant (hills) scenic amenity overlay, roofs and wall surfaces of buildings and structures are painted or finished such that reflectivity is less than 35%.  |  |  |
| **PO66**Landscaping1. complements the coastal landscape character and amenity;
2. has known resilience and robustness in the coastal environment;

Fences and walls:1. do not appear visually dominant or conspicuous within its setting;
2. reduce visual appearance through the use of built form articulation, setbacks, and plant screening;
3. use materials and colours that are complementary to the coastal environment.

Building design responds to the bayside location and complements the particular bayside character and amenity by adopting and incorporating a range of architectural character elements. Vegetation that contributes to bayside character and identity are: 1. retained;
2. protected from development diminishing their significance.
 | **E66**Where located in the Locally Important (Coast) scenic amenity overlay:1. landscaping comprises indigenous coastal species;
2. fences and walls are no higher than 1m; and
3. existing pine trees, palm trees, mature fig and cotton trees are retained.
4. where over 12m in height, the building design includes the following architectural character elements:
	1. curving balcony edges and walls, strong vertical blades and wall planes;
	2. balcony roofs, wall articulation expressed with different colours, curves in plan and section, and window awnings;
	3. roof top outlooks, tensile structures as shading devices;
	4. lightweight structures use white frame elements in steel and timber, bold colour contrast.
 |  |  |
| **Transport noise corridors (refer Overlay map - Transport noise corridors to determine if the following assessment criteria apply)**

|  |
| --- |
| Note - This is for information purposes only. No requirements for accepted development or assessable criteria apply. Development located within a Transport Noise Corridor must satisfy the requirements of the Queensland Development Code  |

 |

**Setback Tables**

|  |
| --- |
| **Table 9.3.1.3 Setbacks** |
| **Coastal communities precinct and Redcliffe Kippa-Ring local plan - Interim residential precinct** |
| **Height of wall** | **FrontagePrimary** | **FrontageSecondary to street** | **Frontage Secondary to lane** | **Side To OMP and wall** | **Rear To OMP and wall** | **Canal To OMP and wall** |
| **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note -  These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To OMP, wall and covered car parking space** |
| **Less than 4.5m** | Min 6m | Min 4.5m | Min 5.4 | Min 3m | Min 2m | Min 5.4 | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **4.5m to 8.5m** | Min 6m | Min 4.5m | N/A | Min 3m | Min 2m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **Greater than 8.5m** | Min 6m | Min 4.5m | N/A | Min 3m | Min 2m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |

|  |
| --- |
| **Table 9.3.1.4 Setbacks** |
| **General residential zone - Suburban neighbourhood precinct and Township zone - Residential precinct** |
| **Height of wall** | **FrontagePrimary** | **FrontageSecondary to street** | **FrontageSecondary to lane** | **SideNon-built to boundary wall To OMP and wall** | **Rear To OMP and wall** | **Canal To OMP and wall** |
| **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note -  These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To OMP**, **wall and covered car parking space** |
| **Less than 4.5m** | Min 4.5m | Min 3m | Min 5.4 | Min 3m | Min 2m | Min 5.4 | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **4.5m to 8.5m** | Min 4.5m | Min 3m | N/A | Min 3m | Min 2m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **Greater than 8.5.** | Min 4.5m | Min 3m | N/A | Min 3m | Min 2m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |

|  |
| --- |
| **Table 9.3.1.5 Setbacks** |
| **Emerging community zone - Transition precinct (developed lot), General residential zone - Next generation neighbourhood precinct and Caboolture West local plan - Urban living precinct (Next generation neighbourhood sub-precinct)** |
| **Height of wall** | **Frontage****Primary** | **Frontage****Secondary to street** | **Frontage Secondary to lane** | **Side****Non-built to boundary wall To OMP and wall** | **Rear To OMP and wall** | **Canal To OMP and wall** |
| **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To OMP**, **wall and covered car parking space** |
| **Less than4.5m** | Min 3m | Min 2m | Min 5.4m | Min 2m | Min 1m | Min 5.4m | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **4.5m to 8.5m** | Min 3m | Min 2m | N/A | Min 2m | Min 1m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **Greater than 8.5m** | Min 6m | Min 5m | N/A | Min 3m | Min 2m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |

|  |
| --- |
| **Table 9.3.1.6 Setbacks** |
| **General residential zone - Urban neighbourhood precinct, and Emerging community zone - Transition precinct (developed lot) and identified in the Morayfield South urban area on Figure 9.3.1.1** |
| **Height of wall** | **Frontage****Primary** | **Frontage****Secondary to street** | **Frontage****Secondary to lane** | **Side****Non-built to boundary wall To OMP and wall** | **Rear To OMP and wall** | **Canal To OMP and wall** |
| **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To wall** | **To OMP** | **To covered car parking space**

|  |
| --- |
| Note - These requirements apply to all Class  10a buildings and structures as defined by the Building Code of Australian. |

 | **To OMP**, **wall and covered car parking spaces** |
| **Less than4.5m** | Min 1m | Min 1m | Min 5.4m | Min 1m | Min 1m | Min 5.4m | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **4.5 to 8.5m** | Min 1m | Min 1m | N/A | Min 1m | Min 1m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |
| **Greater than 8.5m** | Min 5m | Min 3m | N/A | Min 2m | Min 1m | N/A | Min 0.5 | As per QDC | As per QDC | Min 4.5m |

|  |
| --- |
| **Table 9.3.1.7 Built to boundary walls** |
| **Lot frontage width** | **Mandatory / Optional** | **Length and height of built to boundary wall** |
| **General residential zone:*** **Coastal communities precinct**
* **Suburban neighbourhood precinct**

**Redcliffe Kippa-Ring local plan:*** **Interim residential precinct**
 | **Emerging community zone:*** **Transition precinct (Developed lot)**

**General residential zone:*** **Next generation neighbourhood precinct**

**Caboolture West local plan:*** **Urban living precinct (Next generation sub-precinct)**
 | **Emerging community zone:*** **Transition precinct (Developed lot) if within the Morayfield South urban area on Figure 9.3.1.1**

**General residential zone:*** **Urban neighbourhood precinct**
 |
| **7.5m or less** | Mandatory - both sides unless a corner lot | Not permitted\* | Max Length: 80% of the length of the boundaryMax Height: 7.5m  | Max Length: 80% of the length of the boundaryMax Height: 8.5m  |
| **More than 7.5m to 12.5m** | Mandatory - one side | Not permitted\* | Max Length: 60% of the length of the boundaryMax Height: 7.5m  | Max Length: 70% of the length of the boundaryMax Height: 10.5m  |
| **More than 12.5m to 18m** | Optional:1. on 1 boundary only;
2. where the built to boundary wall adjoins a lot with a frontage less than 18m.

Not permitted - Otherwise | Not permitted\* | Max Length: the lesser of 15m or 60% of the length of the boundaryMax Height: 7.5m  | Max Length: the lesser of 15m or 60% of the length of the boundaryMax Height: 10.5m  |
| **Greater than 18m** | Not permitted\* | Not permitted\* | Not permitted\* | Not permitted\* |

|  |
| --- |
| Note -The above setbacks apply only to Class 1a and Class 10a buildings/structures.Note - Max Length includes the length of walls of any other buildings on the same boundary. e.g. detached garage, carport or shed. Note - For the maximum height of domestic outbuildings refer to the examples that achieve aspects of the performance outcomes for building height and domestic outbuildings. \*Note - Built to boundary walls are not permitted, however, reduced side and rear boundary clearances may be permitted as prescribed (e.g. QDC).   |

**Figure 9.3.1.1 Morayfield South - Urban area**

