|  |
| --- |
| **Table 9.4.2.1 Requirements for accepted development  - Works** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for accepted development** | | **E Compliance**   * **Yes** * **No** | **Council confirmation** |
| **Works within a non-tidal artificial waterway** | |  |  |
| **RAD1** | Pontoons, jetty’s and berthed vessels are setback a minimum of 1.5 metres from the water allocation side boundaries. |  |  |
| **RAD2** | Boardwalks and decks are setback a minimum of 3 metres from the prolongation of side lot boundaries and extend no more than 3 metres seaward of the property boundary. |  |  |
| **RAD3** | Pontoons, jetty's, boardwalks and decks are not roofed. |  |  |
| **RAD4** | The underside of the jetty/gangway is a maximum of 300mm above the height of the revetment wall. |  |  |
| **RAD5** | All lighting, other than an aid to navigation, is hooded and directed downwards. |  |  |